
Q2-1.

Z = 144 pins


I = 2048 Kbytes of Flash memory

T = LQFP

6 = Industrial temperature range, -40 to 85 degrees Celsius




Q2-2. The allowable maximum current consumption by the Nucleo-F767ZI board when the U5V input is chosen is 500 mA.



Q2-3.

Page 466/1954 from Ref\_03\_RM0410 Reference Manual\_STM32F76xxx\_R4\_Mar2018.pdf



Page 168/252 from Ref\_02-1\_DS11532\_Datasheet STM32F767xx\_stm32f767zi\_R7\_Feb2021.pdf

